

**PCB Specification FC-Sensor**

* Board Layer Stackup




* Constraints




* 120ohm impedance control


It’s necessary to apply 120ohm impedance control to the following CAN traces on the layer3(signal1).



* Assembly

Pin1 indicators





Drawings

