

**PCB Specification Sensornode\_V1.2**

* Board Layer Stackup





* Constraints



* impedance control


It’s necessary to apply 120ohm impedance control to the following CAN traces on the layer3(signal1), layer6(B.Cu).






* Assembly

Pin1 indicators





Drawings

